Basic router configuration:

* Hostname: R1
* Passwords:
* Secret: cisco
* VTY 0 15: cisco
* Console 0: cisco
* Ip address: fe 0/0 192.168.1.1/24 description Lan to S1 no shut
* Fe 0/1 192.168.2.1/24 description Lan to S2 no shut
* Service password-encryption
* Banner motd “No Authorized Access”:

Switch Olya: vlan 1 ip address 192.168.1.2/24 S1

* Default gate-way: router ip
* Hostname: S1
* General password: cisco
* telnet via: 23192.168l
* close all ports
* logging synchronous

Switch Son vlan 1 ip address 192.168.2.2/24 S2

* Default gate-way: router ip
* Hostname: S2
* General password: cisco
* telnet via: 23
* close all ports
* logging synchronous

Hostname: S2

* General password: cisco

PC Son: 192.168.1.10/24

Pc Olya:192.168.2.10/24